Method for aligning spots on camera for 6 beams configuration

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Step** | **Open Shutter** | **Spot** | **Pico [alternate]** | **Comments (To be confirmed)** |
| 1 | B1 | L1 | Dicroic 1 (or T3H) | top spot |
| 2 | B1 | R2 | T2H | top spot |
| 3 | B2 | L2 | Dicroic 2 (or T3M) | top spot |
| 4 | B2 | R3 | T2M | bottom spot |
| 5 | B2 | R2 | BC1-2 | top spot |
| 6 | B3 | L3 | Dicroic 3 (or T4H) | bottom spot |
| 7 | B3 | R4 | T1L | top spot |
| 8 | B3 | R3 | BC2-3 | bottom spot |
| 9 | B4 | L4 | Dicroic 4 (T4M) | top spot |
| 10 | B4 | R5 | T1H | bottom spot |
| 11 | B4 | R4 | BC3-4 | top spot |
| 12 | B5 | L5 | Dichroic 5 | top spot |
| 13 | B5 | R6 | T1M | should be clean |
| 14 | B5 | R5 | BC4-5 | bottom spot |
| 15 | B6 | L6 | Dichroic 6 | should be clean |
| 16 | B6 | R1 | T2L | top spot |
| 17 | B6 | R6 | BC5-6 | should be clean |
| 18 | B6 | L1 | BC6-1 |  ??? |

