Prism 1:

Specifications:

Material: IRGn6 glass Diameter: 25mm Diameter tolerance: +0.00/-0.10mm Surface quality: 60-40 Surface accuracy: λ/20 @ 1.5microns	Bevel: 0.3mm x 45° Angle: 6.18° angle tolerance: +/- 30arcsecond Thickness: 2mm Coating: broad band AR, 1.5-2.4microns

T = 2.00mm 4.69mm 6.18degrees D = 25mm

Prism 2:

Specifications:

Material: IRGn6 glass Diameter: 25mm Diameter tolerance: +0.00/-0.10mm Surface quality: 60-40 Surface accuracy: λ/20 @ 1.5microns	Bevel: 0.3mm x 45° Angle: 17.5° angle tolerance: +/- 30arcsecond Thickness: 2mm Coating: broad band AR, 1.5-2.4microns

T = 2.00mm 9.52mm 17.5degrees D = 25mm

2005-06-07T18:48:05